Ethernet

MZF XLR 1 - Ground (black) 3

MZF XLR 2 - Positive (red) 1

MZF XLR 3 - Negative (blue) 2

MZF XLR S – Shield (brown) S

FZF XLR 1 - Ground (black) 3

FZF XLR 2 - Positive (red) 4

FZF XLR 3 - Negative (blue) 5

FZF XLR S – Shield (brown) S

M perch sense – signal (yellow) 6

M perch sense – power (red) 7

M perch sense – ground (black) 3

F perch sense – signal (yellow) 8

F perch sense – power (red) 7

F perch sense – ground (black) 3